The Gugusse Compact is an upgrade from the Gugusse Roller.

  The Gugusse Compact base combines in a single piece what was 3 pieces in the Gugusse Roller; the Tensioner Base, the Gate Base and the Main Drive

.  The Gugusse Roller's adjustable Gate Jaws and hole sensor are now replaced by non-adjustable but swappable Gates and hole sensors, you have to print one of each for each film format you wish to scan.



The rollers are now fixed size, you need to print 8 for each film format you wish to scan (8mm and super8 share the same rollers, but not the same gate and not the same hole sensor).



You need to make 2 turntables (like the old Gugusse Roller).  

You need to make a controlboard (like the old Gugusse Roller).  

You need to print 1 BigSwivelArm.stl but 2 SmallSwingingArm.stl.  35mm doesn't need ReelRaisers but the other formats do, you'll need to print 2 for each format you'll scan.





Find more information about the (now old) Gugusse Roller at:
www.deniscarl.com. Beware the documentation will not be updated to the
Gugusse Compact version for a while, until then come and see us at
 https://www.facebook.com/groups/552059449113276 for questions.





