The files in this folder have been modified from the official parts supplied for the Gugusse Compact by Al Warner.

Included are:

Reel Raisers for 8mm and 16mm film with the addition of a small hole on one side.  You can use this to insert a small pin
in the hole to act as a key to move the film.  I use a pin from a .156 header connector.  See DigiKey A19893-ND as
an example.  But a cut paperclip might work as well.

A shorter Glissade.  This will fit on a 256x256 print surface and is big enough for all focal lengths using the standard lens.

Turntable Shoe 2 which has indents to allow the two lower screws to be used on the turntable base motor plate.



