The Gugusse Compact is a DIY motion picture film scanner designed by Denis-Carl Robidoux

The scanner uses swappable Gates and hole sensors, you have to print one of each for each film format you wish to scan.

You need to print 8 rollers for each film format you wish to scan (8mm and Super-8 share the same rollers, but not the same gate and not the same hole sensor).

You need to make 2 turntables.  

You need to make a controlboard (New Design Included).  

You need to print 1 BigSwivelArm.stl but 2 SmallSwingingArm.stl.  35mm doesn't need ReelRaisers but the other formats do, you'll need to print 2 for each format you'll scan.


Find more information about the Gugusse Compact at: www.deniscarl.com. 
Come and see us at: https://www.facebook.com/groups/552059449113276 for questions.





